INSERT PICTURE OF MACHINE HERE WITH LOCK OUT INFORMATION HIGHLIGHTED

**GUIDELINES PROHIBIT HANDS / FINGERS IN AREA OF OPERATIONS**

**(ALL PROCEDURES ARE MACHINE SPECIFIC)**

|  |  |  |
| --- | --- | --- |
| **Hazards Present:** | **Personal Protective Equipment or Devices Required:** | **Training Requirements:** |
| * Awkward/Sustained Postures * Forceful Exertions * Repetitive Movements * Vibration * Compression * Sharp Points/Edges * Pinch/Crush Points * Falling Materials * Uneven Surfaces * Moving Machinery * Chemicals * Biological Pathogens * Electrical * Extreme Heat/Cold * Noise * Combustibles/Flammables * Burns/Fire * Welders Flash * Other - | * Hard Hat * Face Shield * Safety Glasses * Hearing Protection – Plugs or Muffs * Double Hearing Protection – Plugs and Muffs * CSA Grade 1 safety toe boots * Leather Gloves * Aluminized Neck Drape * Cold Vest * N95 Dust Mask * Half Mask Respirator With P100 Filters | * Confined Space Entrant * Confined Space Attendant * Fork Truck Certified * Aerial Lift Certified * Medical Examination * Fit Test |
| **Safe Work Procedure:** | | |
| 1. Before beginning this job, check and put on all required PPE. | | |
| ***If an emergency situation occurs while conducting this task, or there is an equipment malfunction, engage the emergency stop.*** | | |
| **REPORT ANY HAZARDOUS SITUATIONS TO YOUR SUPERVISOR OR DESIGNATE IMMEDIATELY** | | |
| Guidance Documents / Standards / Applicable Legislation / Other: | | |
| **Manitoba Workplace Safety and Health Regulation, M.R. 217/2006 with updates in 2014.** | | |
| **CSA Standards:** | | |
|  | | |
|  | | |
|  | | |
|  | | |
| **This Safe Work Procedure will be reviewed at a minimum of every three years as well as any time the task, equipment or materials change.** | | |