INSERT PICTURE OF MACHINE HERE WITH LOCK OUT INFORMATION HIGHLIGHTED

**GUIDELINES PROHIBIT HANDS / FINGERS IN AREA OF OPERATIONS**

**(ALL PROCEDURES ARE MACHINE SPECIFIC)**

|  |  |  |
| --- | --- | --- |
| **Hazards Present:** | **Personal Protective Equipment or Devices Required:** | **Training Requirements:** |
| * Awkward/Sustained Postures
* Forceful Exertions
* Repetitive Movements
* Vibration
* Compression
* Sharp Points/Edges
* Pinch/Crush Points
* Falling Materials
* Uneven Surfaces
* Moving Machinery
* Chemicals
* Biological Pathogens
* Electrical
* Extreme Heat/Cold
* Noise
* Combustibles/Flammables
* Burns/Fire
* Welders Flash
* Other -
 | * Hard Hat
* Face Shield
* Safety Glasses
* Hearing Protection – Plugs or Muffs
* Double Hearing Protection – Plugs and Muffs
* CSA Grade 1 safety toe boots
* Leather Gloves
* Aluminized Neck Drape
* Cold Vest
* N95 Dust Mask
* Half Mask Respirator With P100 Filters
 | * Confined Space Entrant
* Confined Space Attendant
* Fork Truck Certified
* Aerial Lift Certified
* Medical Examination
* Fit Test
 |
| **Safe Work Procedure:** |
| 1. Before beginning this job, check and put on all required PPE.
 |
| ***If an emergency situation occurs while conducting this task, or there is an equipment malfunction, engage the emergency stop.***  |
| **REPORT ANY HAZARDOUS SITUATIONS TO YOUR SUPERVISOR OR DESIGNATE IMMEDIATELY** |
| Guidance Documents / Standards / Applicable Legislation / Other: |
| **Manitoba Workplace Safety and Health Regulation, M.R. 217/2006 with updates in 2014.** |
| **CSA Standards:** |
|  |
|  |
|  |
|  |
| **This Safe Work Procedure will be reviewed at a minimum of every three years as well as any time the task, equipment or materials change.**  |